**Make: Wilkhahn**

**Model: Confair flip-top tables, nest into one another**

Design: Andreas Störiko

  

**Models:**

440/00 rectangular

440/2 curved on the long sides

**Standards:**

ANSI / BIFMA X 5.5

**Table dimensions:**

Height to top edge of table top: 73 cm

Depth x width:

Model 440/00 rectangular
90 x 180 / 200 / 210 / 220 / 240 / 260 / 280 / 300 cm

100 x 180 / 200 / 210 / 220 / 240 / 260 / 280 / 300 cm

105 x 180 / 200 / 210 / 220 / 240 / 260 / 280 cm

110 x 180 / 200 / 210 / 220 / 240 / 260 / 280 cm

120 x 180 / 200 / 210 / 220 / 240 / 260 cm

Model 440/2 curved on the long sides

90/110 x 260 cm

90/120 x 180 / 240 / 260 / 280 cm

**Weight:**

Size 90 x 260 cm: 65.23 kg (depending on the model and design without packaging)

**Function:**

Mobile table range with table tops that can be flipped up on their horizontal axes, table tops partitioned in the middle for versatile use in conference, presentation and meeting rooms, as well as in multi-purpose areas and office environments.

When flipped up, tables nest into one another and save space, dimensions when flipped up: approx. 20 cm per table (measured from the middle axis of each table to the next).

The table top can be flipped up easily with both hands and without any tools required. Swivel the table top downwards by just pressing down on it. It doesn’t have to be locked in place in either position.

**Frame:**

Foot section made of die-cast aluminium, coated (black or silver satin finish)

Optional: Foot section bright chrome-plated or polished

Upright made of aluminium profile coated (black or silver satin finish)

Optional: Clear anodised or bright chrome-plated upright

Uprights made of aluminium profile, coated (black or silver satin finish) Clear anodised uprights
Connecting bar, coated (black or silver satin finish)
Optional: connecting bar bright chrome plated (only when combined with a chrome-plated foot section and upright)

Lockable castors with tyre made of black polyamide, 10 cm in diameter

**Table top:**

Laminboard class E1

Concealed wood lipping all the way round, optionally bullnose wood or straight lipping, with integral, impact-resilient profile in black elastomer

Edge profiles:



**Table top surface:**

Table top group 1– laminate

Table top thickness 26 mm

Laminate based on Wilkhahn colour and surface finish samples with laminated beech lipping, natural oiled finish

Table top group 2 – veneer

Table top thickness 26 mm

Variation 1:

Beech veneer based on Wilkhahn colour and surface finish samples with laminated beech lipping, oak or ash veneer based on Wilkhahn colour samples with lipping, as far as possible to colour-match the veneer

Variation 2:

Maple, walnut or elm veneer, as well as Wilkhahn Mocca veneer from the Wilkhahn colour samples with lipping as far as possible in the same colour as the veneer

Veneer types:

As a standard, the veneers are produced using the slip-match method

Some specific growth features are possible

Surfaces sealed with clear lacquer:

Open-pore: oak, ash, walnut and elm veneer, as well as Wilkhahn Mocca veneer

Closed-pore: maple and beech veneer

Table top group 3 – linoleum:

Table top thickness 27 mm

Linoleum from the Wilkhahn colour samples, with laminated beech lipping, natural oiled finish

Optional: Customised options possible on request. Shapes, dimensions, surfaces and edges after feasibility has been tested

Special designs to suit customer’s preferences after clarifying technical details with Wilkhahn

**Environmental product information:**

Materials used in size 90 x 260 cm: wood 68.43%, steel 6.48% aluminium 20.73%, plastics 4.16%

Returns, disassembly and recycling:

All Confair flip-top table components can be dismantled non-destructively.

To ensure that materials can be sorted according to type, all components weighing more than 150 g have been labelled accordingly. No agents to protect materials or organic halogen compounds are used which would prevent subsequent recycling. In total 90 per cent of the table can be recycled.

For more information see: http://www.wilkhahn.com/green

**Accessories:**

Optional: Table-table-connectors (model 613): two swivel-mounted, lockable circlips made of black-coated sheet steel with four star-grip screws

Optional: Integrated techni-station Rotate with 3 modules (model 701/60), 4 modules (model 701/70), or integrated techni-station Compact with 3 modules (model 701/95). Clear anodised aluminium body, sides made of plastic similar to RAL 9006, black plastic modules, swivel-mounted frame, pre-wired and prepared for assembly, with cables

Optional: single table portal set with brush profile: Portal the same colour and material on both sides, flush with the table surface, cut-out section on the table top with genuine wood lipping all around, as far as possible in the same colour as the table top, with hinges that open 180°, single table portal dimensions: 300 x 150 mm. Cable basket for assembly underneath the table top (for inserting outside the underframes), or storage mesh (for inserting within the underframes). Mount (metal bracket) for power strips. Cable clips made of black, glass fibre-reinforced polyamide to accommodate the vertical cable management system on the table frame’s upright

Optional: Single table portal Basic set: Clear anodised aluminium body, with portal and brushed profile, frame placed on the table top, opening angle 90°. Single table portal Basic dimensions: 300 x 120 mm. Cable basket for assembly underneath the table top (for inserting outside the underframes), or storage mesh (for inserting within the underframes). Mount (metal bracket) for power strips. Cable clips made of black, glass fibre-reinforced polyamide to accommodate the vertical cable management system on the table frame’s upright

Optional: Socket strip (models 708/1, 708/2, 708/4, 708/5, 708/6), 3-5 modules can be selected with various configurations comprising electricity and/or data, and/or VGA, with the appropriate leads

Optional: Supply cable, 3 x 1.5 mm², black, Schuko right angle plug + jack GST18/3, length approx. 300 cm (model 708/8) or extension lead, 3 x 1.5 mm², black, plug + jack GST18/3, length approx. 100 cm (model 708/9)

On request multi-media equipment can be integrated when table top group 3 is chosen

**Certificates and awards for Confair folding table**

UN Global Compact

ISO 9001

ISO 14001

EMAS
FSC

GREENGUARD™ (undergoing certification)

LEED

The following LEED rating can be achieved:

LEED CI 5 – 7

LEED NC 4

LEED EB 7

**International design awards for the Confair flip-top table:**

1995: Design-Week Award, United Kingdom, 1st prize

1995: Best of Competition, Apex Award, International Interior Design Association Chicago/US

1996: Goed Industrieel Ontwerp / Netherlands “Best of Category”

1996: Industrie Forum Design, Good Design, “The Best in the Industry”, Hanover, Germany

1996: Design Center NRW, “Red dot for high-quality design”, Essen, Germany

1996: Industrial Design Excellence Award, “Silver” in the furniture category, Industrial Designers Society of America and Business Week

1996: Design Center NRW, Top design quality for the flip-top table, “The best of the best” Essen, Germany

1997: Aluminium Award, Netherlands Aluminium Centrum

1998: Compasso d’oro, Milan, Italy

2000: Architektur und Office innovation prize, AIT, Orgatec, Cologne, Germany

2004: Anniversary Award “10 of 50”, winner of office-furniture systems, md International magazine of design

Wilkhahn reserves the right to make technical changes to the information provided.

Published in November 2015